|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 500 – Channel without inbuilt fall** + Length 1000 mm / 2000 mm+ Width at angle 650 mm, width at bottom 700 mm+ Construction height 655 mmmade of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOsir NW 500 channel[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to the installation instructions of the producer.Producer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir NW 500 End caps and end caps with outlet DN 300**+ Width 650 mm+ For construction height 655 mmmade of galvanized steel[ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0[ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 300 for channel  no. 0/0delivery.Producer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 500 – Grating**+ Width 633 mm+ Height 45 mmload class according to DIN EN 1433, with 8 point per meter M16/A2-bolt fastening or Easylock fastening [ ] \_\_\_\_\_ pce ductile iron threefold slotted gratings, black immersion- lacquered, length 500 mm, load class  D 400 / E 600 / F 900delivery and installation according to the installation instructions of the producer Producer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 500 – Cutting of channels including grating** and painting or galvanizing of cutted angles and gratings.[ ] \_\_\_\_\_ Channel section 90°[ ] \_\_\_\_\_ Mitre cut according to degree specificationProducer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 500 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300delivery.Producer: BIRCO GmbH | **Unit price** | **Total price** |