|  |  |  |
| --- | --- | --- |
| **BIRCOsir Point Drainage 30/30 – Outfall unit** alsofor drainage channel connection on two sides (NW 100)+ Length at angle frame 300 mm/ Length at bottom 320 mm+ Width at angle frame 300 mm/ Width at bottom 320 mm+ PP odour trap+ PP silt bucket+ Integrated socket for DN 100 pipe connectionmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ pce outfall unit, 1 piece, construction height 420 mm[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir Point Drainage 30/30 – Gratings**+ Width 280 mm+ Height 30 mmload class according to DIN EN 1433, with 2-point per grating M12/A2-bolt fastening or Easylock fastening [ ] \_\_\_\_\_ pce ductile iron twofold slotted grating black  immersion-lacquered, length 280 mm, load class E 600[ ] \_\_\_\_\_ pce mesh grating galvanized steel,  length 280 mm, mesh width 30/30 mm / 30/15 mm, load class C 250delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir Point Drainage 40/40 – Outfall unit, 1-piece** alsofor drainage channel connection on three sides (NW 100 and 150)+ Length at angle 400 mm/ Length at bottom 415 mm+ Width at angle frame 400 mm/ Width at bottom 415 mm+ PP odour trap+ PP silt bucket+ Integrated socket for DN 150 pipe connectionmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ pce outfall unit, 1 piece, construction height 575 mm[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-47; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir Point Drainage 40/40 – outfall unit, 2-piece**+ Length at angle 400 mm/ Length at bottom 410 mm+ Width at angle frame 400 mm/ Width at bottom 410 mm+ PP odour trap+ PP silt bucket+ Integrated socket for DN 200 pipe connectionmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ pce outfall unit, 2-piece, construction height 880 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir Point Drainage 40/40 – outfall unit, 3-piece**alsofor drainage channel connection on four sides (NW 100, NW 150, NW 200 to no. 20)+ Length at angle 400 mm / Length at bottom 410 mm+ Width at angle frame 400 mm/ Width at bottom 410 mm+ PP odour trap+ PP silt bucket+ Integrated socket for DN 200 pipe connectionmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ pce outfall unit, 3-piece, construction height 1200 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir Point Drainage 40/40 – Gratings**+ Width 380 mm+ Height 40 mmload class according to DIN EN 1433, with 4-point per grating M12/A2-bolt fastening or Easylock fastening [ ] \_\_\_\_\_ pce ductile iron twofold slotted grating black immersion- lacquered, length 380 mm, load class E 600[ ] \_\_\_\_\_ pce mesh grating galvanized steel,  length 380 mm,  mesh width 30/30, load class C 250 mesh width 30/15, load class C 250 mesh width 20/30, load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |