|  |  |  |
| --- | --- | --- |
| **BIRCOsir Rail track drainage rail profile 49E1/54E3  (old designation: S 49/S 54)**  + Channel BIRCOsir NW 100, no. 0/0  + 2-piece  + Two-sided rail track drainage casings for collecting surface   water  + Ductile iron slotted grating black immersion-lacquered  + 8-point per metre M12/A2-bolt fastening  + Integrated sockets for DN 100 pipe connection DN 100  [ ] \_\_\_\_\_ pce tail track drainage, gauge 1435 mm,   construction height 180 mm  [ ] Sealing with SF-Connect  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir Rail track drainage rail profile 57R1/67R1  (old designation: Ph37/Ph37a)**  + Channel BIRCOsir NW 100, no. 0/0  + 3-piece  + Two-sided rail track drainage casings for collecting surface   water  + Ductile iron slotted grating black immersion-lacquered  + 8-point per metre M12/A2-bolt fastening  + Integrated sockets for DN 100 pipe connection DN 100  [ ] \_\_\_\_\_ pce tail track drainage, gauge 1435 mm  construction height 180 mm  [ ] Sealing with SF-Connect  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-47; www.birco.de | **Unit price** | **Total price** |