|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler DN 400 – channel element type I without inbuilt fall, ASR resistant**+ Monolithic concrete body+ Length 4000 mm+ Width at top 570 mm, width at bottom 610 mm+ Construction height 585 mm+ Cross sectional area: 1256 cm²made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 400, load class D 400,  intermittent slot, slot width 30/50 mm, inclined surface  to the slot[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 400, load class F 900,  intermittent slot, slot width 30/50 mm, inclined surface  to the slot[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 400, load class D 400  / F 900, length \_\_\_\_\_\_\_ mm (between 250 and 3950  mm, to enquire about)[ ] Channel with integrated kerb[ ] Sealing with lubricant DENSOdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler DN 400 – channel element with outlet, type I, ASR resistant**+ Monolithic concrete body+ Length 1000 mm+ Width at top 570 mm+ Total height 1295 mmmade of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433Channel element with vertical outlet DN 300, silk bucket and ductile iron grating[ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Pfuhler  DN 400, load class D 400, with inclined surface the slot[ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Pfuhler  DN 400, load class F 900, with inclined surface the slot[ ] Sealing with lubricant DENSOdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Pfuhler DN 400 – inspection channel, type I without inbuilt fall, ASR resistant**+ Monolithic concrete body+ Length 1000 mm+ Width at top 570 mm, width at ground 610 mm+ Total height 585 mmmade of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433 and ductile iron grating[ ] \_\_\_\_\_ pce inspection channel Pfuhler DN 400, load class  D 400, with inclined surface to the slot[ ] \_\_\_\_\_ pce inspection channel Pfuhler DN 400, load class  F 900, inclined surface to the slot[ ] Sealing with lubricant DENSOdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Pfuhler DN 400 – end cap**Made of concrete[ ] \_\_\_\_\_ pce of end cap female, construction height 585 mm[ ] \_\_\_\_\_ pce of end cap male, construction height 585 mmdelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |