|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler Profile 300/400 – channel element type I without inbuilt fall, ASR resistant**+ Monolithic concrete body+ Length 4000 mm+ Width at top 460 mm, width at bottom 500 mm+ Construction height 600 mm+ Cross sectional area: 1006 cm²made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler Profile 300/400, load  class D 400, intermittent slot, slot width 30/50 mm,  inclined surface to the slot[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler Profile 300/400, load  class D 400, continuous slot, slot width 30/50 mm,  inclined surface to the slot[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler Profile 300/400, load  class F 900, intermittent slot, slot width 30/50 mm,  plane surface[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler Profile 300/400, load  class D 400 / F 900, length \_\_\_\_\_\_\_ mm (between 250  and 3950 mm, to enquire about)[ ] Channel with integrated kerb[ ] Sealing with lubricant DENSOdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler Profile 300/400 – channel element type I with inbuilt fall, ASR resistant**+ Monolithic concrete body+ Length 4000 mm+ Width at top 460 mm, width at bottom 500 mm+ Construction height 600 mm+ Cross sectional area: 766 to 1006 cm²made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler Profile 300/400, channel  no. 1 to 5, load class D 400, intermittent slot, slot  width 30/50 mm, inclined surface to the slot[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler Profile 300/400, channel  no. 1 to 5, load class D 400, continuous slot, slot width  30/50 mm, inclined surface to the slot[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler Profile 300/400, channel  no. 1 to 5, load class F 900, intermittent slot, slot  width 30/50 mm, plane surface[ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler Profile 300/400, channel  no. 1 to 5, load class D 400 / F 900, length \_\_\_\_\_\_\_  mm (between 250 and 3950 mm, to enquire about)[ ] Channel with integrated kerb[ ] Sealing with lubricant DENSOdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler Profile 300/400 – channel element with outlet, type I, ASR resistant**+ Monolithic concrete body+ Length 1000 mm+ Width at top 460 mm+ Total height 1310 mmmade of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433Channel element with vertical outlet DN 300, silk bucket and ductile iron grating[ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Pfuhler  Profile 300/400, load class D 400, with inclined surface  the slot[ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Pfuhler  Profile 300/400, load class F 900, with plane surface[ ] Sealing with lubricant DENSOdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Pfuhler Profile 300/400 – inspection channel, type I without inbuilt fall, ASR resistant**+ Monolithic concrete body+ Length 1000 mm+ Width at top 460 mm, width at ground 500 mm+ Total height 600 mmmade of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433 and ductile iron grating[ ] \_\_\_\_\_ pce inspection channel Pfuhler Profile 300/400, load  class D 400, with inclined surface the slot[ ] \_\_\_\_\_ pce inspection channel Pfuhler Profile 300/400, load  class F 900, with plane surface[ ] Sealing with lubricant DENSOdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Pfuhler Profile 300/400 – end cap**+ for channels without inbuilt fallMade of galvanized steel[ ] \_\_\_\_\_ pce of end cap, construction height 600 mmdelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler Profile 300/400 – end cap**+ for channels with inbuilt fallMade of concrete[ ] \_\_\_\_\_ pce of end cap female, construction height 600 mm[ ] \_\_\_\_\_ pce of end cap male, construction height 600 mmdelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |