|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Solidrain S DN 200 – channel element type I without inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 4000 mm  + Width at top 330 mm, width at bottom 360 mm  + Construction height 330 mm  + Cross sectional area: 314 cm²  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  [ ] \_\_\_\_\_ m BIRCOslot channel Solidrain S DN 200, load class   C 250, intermittent slot, slot width 30/50 mm, inclined   surface to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Solidrain S DN 200, load class   C 250, length \_\_\_\_\_\_\_ mm (between 250 and 3950   mm, to enquire about)  [ ] Channel with integrated kerb  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOslot channel Solidrain S DN 200 – channel element with outlet, type I, ASR resistant**  + Monolithic concrete body  + Length 1000 mm  + Width at top 330 mm  + Total height 930 mm  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  Channel element with vertical outlet DN 200, silk bucket and ductile iron grating  [ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Solidrain S   DN 200, load class C 250, with inclined surface the slot  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Solidrain S DN 200 – inspection channel, type I without inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 1000 mm  + Width at top 330 mm, width at ground 360 mm  + Total height 300  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433 and ductile iron grating  [ ] \_\_\_\_\_ pce inspection channel Solidrain S DN 200, load class   C 250, with inclined surface the slot  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Solidrain S DN 200 – end cap**  Made of galvanized steel  [ ] \_\_\_\_\_ pce of end cap, construction height 300 mm  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |