|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Solidrain S Profile 300/400 – channel element type I without inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 4000 mm  + Width at top 420 mm, width at bottom 460 mm  + Construction height 530 mm  + Cross sectional area: 1006 cm²  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  [ ] \_\_\_\_\_ m BIRCOslot channel Solidrain S Profile 300/400, load   class C 250, intermittent slot, slot width 30/50 mm,   inclined surface to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Solidrain S Profile 300/400, load   class C 250, length \_\_\_\_\_\_\_ mm (between 250 and   3950 mm, to enquire about)  [ ] Channel with integrated kerb  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOslot channel Solidrain S Profile 300/400 – channel element type I with inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 4000 mm  + Width at top 420 mm, width at bottom 460 mm  + Construction height 530 mm  + Cross sectional area: 766 to 1006 cm²  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  [ ] \_\_\_\_\_ m BIRCOslot channel Solidrain S Profile 300/400,   channel no. 1 to 5, load class C 250, intermittent slot,   slot width 30/50 mm, inclined surface to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Solidrain S Profile 300/400,   channel no. 1 to 5 load class C 250, length \_\_\_\_\_\_\_   mm (between 250 and 3950 mm, to enquire about)  [ ] Channel with integrated kerb  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Solidrain S Profile 300/400 – channel element with outlet, type I, ASR resistant**  + Monolithic concrete body  + Length 1000 mm  + Width at top 420 mm  + Total height 1240 mm  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  Channel element with vertical outlet DN 300, silk bucket and ductile iron grating  [ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Solidrain S   Profile 300/400, load class C 250, with inclined surface   the slot  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Solidrain S Profile 300/400 – inspection channel, type I without inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 1000 mm  + Width at top 420 mm, width at ground 460 mm  + Total height 530 mm  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433 and ductile iron grating  [ ] \_\_\_\_\_ pce inspection channel Solidrain S Profile 300/400, load   class C 250, with inclined surface the slot  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Solidrain S Profile 300/400 – end cap**  + For channel elements without inbuilt fall  Made of galvanized steel  [ ] \_\_\_\_\_ pce of end cap, construction height 530 mm  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Solidrain S Profile 300/400 – end cap**  + For channel elements with inbuilt fall  Made of concrete  [ ] \_\_\_\_\_ pce of end cap female, construction height 530 mm  [ ] \_\_\_\_\_ pce of end cap male, construction height 530 mm  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |