|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 160 Series without visible edge – Drainage channel**  + Perforated on one side  + Bolt connection bar  + Length 500 / 1000 / 3000 mm  + Width at top 160, at bottom 136 mm  + Construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop F 160, channel construction 50/75  length 500/1000/3000 mm, load class walkable  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 160 Series – End caps**  + Width 100 mm  + For construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop F 130 end cap for construction height   50 / 75 mm  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop F 160 Series – Grating**  + Width 153 mm  + Height 20 mm  With 2-point per metre M12/A2 bolt connection  [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,   length 500 / 1000 mm, mesh width 30/10, load class   walkable  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 160 Series with visible edge – Drainage channel**  + Perforated on two sides  + With and without out bolt connection  + Length 500 / 1000 / 3000 mm  + Width at top 160 mm, width at bottom 100 mm  + Construction height 50 / 75 / 100 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop F 160, channel construction height   50/75/100 with bolt connection, load class walkable  [ ] \_\_\_\_\_ pce BIRCOtop F 160, channel construction height   50/75/100 without bolt connection, load class walkable  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 160 Series - End caps**  + Width 160 mm  + For construction height 50 / 75 / 100 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop F 160 end cap for construction height   50/75/100 mm  delivery and installation according to manufacturers installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop F 160 Series– Gratings**  + Width 158 mm  + Height 20 mm  [ ] \_\_\_\_\_ pce slot grating made of hot-dipped   galvanized steel, clamped grating without bolt   connection, length 500 / 1000 mm,   load class walkable  [ ] \_\_\_\_\_ pce ductile iron slot grating with 2-point per meter   M10/A2 bolt connection, length 500 mm, load class   walkable  [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,   clamped grating without bolt connection  length 500 / 1000 mm, mesh width 30/10 / 30/16  load class walkable  delivery and installation according to manufacturers installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |