|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 210 Series without visible edge – Drainage channel**+ Perforated on one side+ Bolt connection bar+ Length 500 / 1000 / 3000 mm + Width at top 208, at bottom 184 mm+ Construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 210, channel construction 50/75 load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 210 Series – End caps**+ Width 183 mm+ For construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 130 end cap for construction height  50 / 75 mmdelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop F 210 Series – Gratings**+ Width 200 mm+ Height 20 mmWith 2-point per metre M12/A2 bolt connection [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,  length 500 / 1000 mm, mesh width 30/10  load class walkabledelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |