|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 210 Series without visible edge – Drainage channel**  + Perforated on one side  + Bolt connection bar  + Length 500 / 1000 / 3000 mm  + Width at top 208, at bottom 184 mm  + Construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop F 210, channel construction 50/75  load class walkable  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 210 Series – End caps**  + Width 183 mm  + For construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop F 130 end cap for construction height   50 / 75 mm  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop F 210 Series – Gratings**  + Width 200 mm  + Height 20 mm  With 2-point per metre M12/A2 bolt connection  [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,   length 500 / 1000 mm, mesh width 30/10   load class walkable  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |