|  |  |  |
| --- | --- | --- |
| **BIRCOtopline 160 – Drainage channel without visible edge**+ Perforated on one side+ Simple installation from above with plug-in system+ With screw thread for leveling feet+ Length 500 / 1000 / 3000 mm + Width at top 160 mm, at ground 129 mm+ Construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtopline 160, channel construction height  50/75, load class walkable, length 500/1000/3000  mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtopline 160 – corner piece 90 ° without visible edge**+ Perforated on one side+ Simple installation from above with plug-in system+ With screw thread for leveling feet+ Length 500 x 500 mm + Width at top 160 mm, at ground 129 mm+ Construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtopline 160, corner piece 90°, construction  height 50/75, load class walkable, perforation inside /  outsidedelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtopline 160 – End caps**+ Width 160 mm+ For construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtopline 160 end cap for construction height  50 / 75delivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtopline 160 – Gratings with clamping device**+ Width 152 mm+ Height 20 mm+ Load class: walkable[ ] \_\_\_\_\_ pce punched hole grating – circular holes Ø 8 mm, made of galvanized steel, length 500 / 1000 mm[ ] \_\_\_\_\_ pce punched hole grating – square holes 8 x 8 mm, made of galvanized steel, length 500 / 1000 mm[ ] \_\_\_\_\_ pce slot grating made of galvanized steel,  length 500 / 1000 mm[ ] \_\_\_\_\_ pce mesh grating made of galvanized steel,  length 500 / 1000 mm, mesh width 30/10delivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH  | **Unit price** | **Total price** |
| **BIRCOtopline 160 – Gratings with clamping device for corner piece 90°**+ Width 152 mm+ Height 20 mm+ Load class: walkable[ ] \_\_\_\_\_ pce punched hole grating – circular holes Ø 8 mm, made of galvanized steel, length 500 x 500 mm[ ] \_\_\_\_\_ pce punched hole grating – square holes 8 x 8 mm, made of galvanized steel, length 500 x 500 mm[ ] \_\_\_\_\_ pce slot grating made of galvanized steel,  length 500 x 500 mm[ ] \_\_\_\_\_ pce mesh grating made of galvanized steel,  length 500 x 500 mm, mesh width 30/10delivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH  | **Unit price** | **Total price** |
| **BIRCOtopline 160 – Set of leveling feet**+ Galvanized steel+ Set of 4 continuously adjustable leveling feet + Load class: walkable[ ] \_\_\_\_\_ BIRCOtopline 160 set of 4 leveling feetdelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH  | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtopline 160 – Gravel strip**+ Galvanized steel+ For construction height 50 and 75 mm + Width 35 x 45 mm[ ] \_\_\_\_\_ BIRCOtopline 160 gravel strip, length 500 / 1000 mmdelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH  | **Unit price** | **Total price** |