|  |  |  |
| --- | --- | --- |
| **BIRCOmax-i NW 320 – Drainage channel without inbuilt fall, Type I, load class F 900, with cast-in ductile iron angles** + Length 1500 mm / 3000 mm+ With integrated, two-sided anchoring system+ Construction height 600 mm or 800 mm+ Designed for laying from abovemade of concrete C 60/75 according to EN 1433, up to load class F 900 Type I as defined by EN 1433, with anchored 5 mm cast-in ductile iron angles with CDP coating, with 8-point per meter M12/A2 bolt fastening in self-cleaning sockets, with safety sealing joint[ ] \_\_\_\_\_ m BIRCOmax-i channel NW 320, constr. height 600 mm,  width at top/at bottom 504/540 mm,  drainage capacity of 76,67 l/sec, inlet cross section of 1326 cm², retention volume of 132,6 l/m [ ] \_\_\_\_\_ m BIRCOmax-i channel NW 220, constr. height 800 mm, width at top/at bottom 501/504 mm,  drainage capacity of 108,78 l/sec, inlet cross section of 1958 cm², retention volume of 195,8 l/m[ ] Sealing with SF-ConnectDelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfaedel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; [www.birco.com](http://www.birco.com) | **Unit price** | **Total price** |
| **BIRCOmax-i NW 320 – End caps and end caps with outlet DN 300**+ Width 500 mm, made of galvanized steel[ ] \_\_\_\_\_ pce. of end cap(s) for channel construction height 600 / 800 mm [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 315 for channel  construction height 600 / 800Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmax-i NW 320 – Gratings**+ Length 500 mm+ Width 437 mm+ Height 45 mmload class according to EN 1433, with 8-point per meter M12/A2-bolt fastening per meter,[ ] \_\_\_\_\_ pce ductile iron slotted grating, black  immersion lacquered, inlet opening 162/17,5 mm,  inlet cross section 1531 cm²/m,  load class D 400 / E 600 / F 900Delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmax-i NW 320 – PE-foam panel** for expansion joint formation diagonally to the channel line + prefabricated for BIRCOmax-i NW 320 constr. height 800 mm+ adjustable on site if the channel height is lower[ ] \_\_\_\_\_ pce BIRCOmax-i NW 320 PE-foam panelManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmax-i NW 320 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300[ ] \_\_\_\_\_ pce of silt bucket(s)Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmax-i NW 220 – Suspension gear** + Set of 4 pieces+ Load capacity per piece 1 t [ ] \_\_\_\_\_ BIRCOmax-i NW 220 suspension gear, rotatable Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |