|  |  |  |
| --- | --- | --- |
| **BIRCOprofil 160 – Drainage channel**+ With welded-on locking bracket+ With mounting anchor+ Length 500 / 1000 / 3000 mm + Width 160 mm+ Construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOprofil 160, channel construction height  50/75 mm load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOprofil 160 - Connecting shoe**+ Onsite sealing required + Width 160 mm+ for construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOprofil 160 connecting shoe construction  height 50/75 mm[ ] Sealing with SF-Connectdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprofil 160 - End caps**+ Width 160 mm+ For construction height 50 / 75 mm+ Welded on and cold galvanized ex-factorymade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOprofil 160 end cap for construction  height 50/75 mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprofil 160 – Gratings**+ Width 153 mm+ Height 20 mmload class according to EN 1433, with 2-point per metre M12/A2 bolt connection[ ] \_\_\_\_\_ pce cast slotted grating black-immersion lacquered length 500 mm, load class C 250 / E 600[ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,  length 500 / 1000 mm, mesh width 30/15 for  load class C 250 or mesh width 10/30 for load class  E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprofil 160 – Outlet aperture**[ ] \_\_\_\_\_ project-related outlet aperture (for connection to local pipe systemsdelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |