|  |  |  |
| --- | --- | --- |
| **BIRCOprofil 196 - Drainage channel**  + With welded-on bolting device  + With mounting anchor  + Length 500 / 1000 / 3000 mm  + Width 196 mm  + Construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOprofil 196, channel construction height   50/75 mm load class E 600  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOprofil 196 - Connecting shoe**  + Onsite sealing required  + Width 196 mm  + for construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOprofil 196 connecting shoe construction   height 50/75 mm  [ ] Sealing with SF-Connect  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprofil 196 - End caps**  + Width 196 mm  + For construction height 50 / 75 mm  + Welded on and cold galvanized ex-factory  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOprofil 196 end cap for construction   height 50/75 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprofil 196 – Gratings**  + Width 187 mm  + Height 30 mm  load class according to EN 1433, with 2-point per metre M12/A2 bolt connection, mesh grating 4 point fastening per grating  [ ] \_\_\_\_\_ pce cast slotted grating black-immersion lacquered length 500 mm, load class C 250 / E 600  [ ] \_\_\_\_\_ pce. cast mesh gratings black immersion-lacquered, length 500 mm, load class E 600  [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,   length 500 / 1000 mm, mesh width 30/12 mm,   load class C 250  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprofil 196 – Outlet aperture**  [ ] \_\_\_\_\_ project-related outlet aperture  (for connection to local pipe systems  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |