|  |  |  |
| --- | --- | --- |
| **BIRCOprofil 196 - Drainage channel**+ With welded-on bolting device+ With mounting anchor+ Length 500 / 1000 / 3000 mm + Width 196 mm+ Construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOprofil 196, channel construction height  50/75 mm load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOprofil 196 - Connecting shoe**+ Onsite sealing required + Width 196 mm+ for construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOprofil 196 connecting shoe construction  height 50/75 mm[ ] Sealing with SF-Connectdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprofil 196 - End caps**+ Width 196 mm+ For construction height 50 / 75 mm+ Welded on and cold galvanized ex-factorymade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOprofil 196 end cap for construction  height 50/75 mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprofil 196 – Gratings**+ Width 187 mm+ Height 30 mmload class according to EN 1433, with 2-point per metre M12/A2 bolt connection, mesh grating 4 point fastening per grating[ ] \_\_\_\_\_ pce cast slotted grating black-immersion lacquered length 500 mm, load class C 250 / E 600[ ] \_\_\_\_\_ pce. cast mesh gratings black immersion-lacquered, length 500 mm, load class E 600[ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,  length 500 / 1000 mm, mesh width 30/12 mm,  load class C 250delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprofil 196 – Outlet aperture**[ ] \_\_\_\_\_ project-related outlet aperture (for connection to local pipe systemsdelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |