|  |  |  |
| --- | --- | --- |
| **BIRCOcanal – Lifting loops**  + For mechanical installation of concrete covers  + For mechanical installation of supply channels without angles  [ ] \_\_\_\_\_ pce lifting loops RD12 for NW 200 - 500  [ ] \_\_\_\_\_ pce lifting loops RD14 for NW 700 - 1000  Delivery.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal – Side strips**  + As support for BIRCOcanal concrete covers without angles  + Hot-dipped galvanized  + 1 or 2-sided  + Length 1000 mm  + Height 220 mm  [ ] \_\_\_\_\_ pce side strips 1-sided, NW 200 – 700 / NW 1000   material thickness 5 mm  [ ] \_\_\_\_\_ pce side strips 2-sided, NW 200 – 700 / NW 1000   material thickness 5 mm  Delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal – Sealing tape**  + Flexible liner  + Between BIRCOcanal supply channel without angles and   reinforced grade concrete cover  + Self adhesive  [ ] \_\_\_\_\_ m sealing tape, 50/6 mm  Delivery.  Manufacturer BIRCO GmbH | **Unit price** | **Total price** |