|  |  |  |
| --- | --- | --- |
| **BIRCOlight NW 150 AS – Drainage channel with 0.5 % inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 1000 mm  + Width at angle 210 mm, width at bottom 244 mm  + Construction height at groove/tongue 230 to 280 mm  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles and combi-closure toggle, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOlight NW 150 AS channel No. 1 - 10  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOlight NW 150 AS – Drainage channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 500 mm (heights 230 mm)/1000 mm  + Width at angle 210 mm, width at bottom 244 mm  + Construction height 230/255/280/305/325 mm  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles and combi-closure toggle, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOlight NW 100 AS channel No. 0/0, 5/0, 10/0, 15/0, 20/0  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 150 – End caps and end caps with outlet DN 150**  + Width 210 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0 – 4 / 5/0 – 8 / 9 – 10 / 20/0  [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 150 No. 0/0 / 5/0 /   10/0 / 20/0  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOlight NW 150 AS –In-line outfall unit** for 1- or 2-sided channel connection with integrated two-sided anchoring system (AS) made of concrete  + Length at angle 500 mm, length at bottom 510 mm  + Width at angle 210 mm, width at bottom 260 mm,  made of concrete C 40/50 according to EN 1433, PP silt bucket, integrated sockets for DN 100 pipe connection, with anchored 4 mm hot-dipped galvanized solid steel angles (70 µm zinc coating) and combi-closure toggle, with safety sealing joint  [ ] \_\_\_\_\_ pce. In-line outfall unit, single piece, construction   height 710 mm, integrated sockets for DN 150 pipe   connection  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 150 AS – Gratings**  + Width 200 mm  + Height 20 mm  load class according to DIN EN 1433, with 2 point per metre M12/A2-bolt fastening or Easylock fastening  [ ] \_\_\_\_\_ pce. ductile iron slotted gratings black immersion-  lacquered, length 500 mm, load class C 250 / E 600  [ ] \_\_\_\_\_ pce. ductile iron mesh gratings black immersion-  lacquered, length 500 mm, load class C 250 / E 600  [ ] \_\_\_\_\_ pce. mesh grating made of hot-dipped galvanized steel,   mesh width 30/15 mm, length 500 / 1000 mm, load   class C 250  [ ] \_\_\_\_\_ pce. longitudinal bar gratings made of hot-dipped   galvanized steel, length 500 / 1000 mm, load class   C 250  delivery and installation according to manufacturer’s instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 150 AS – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing.  [ ] \_\_\_\_\_ Channel section 90°  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOlight NW 150 AS – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 150  [ ] \_\_\_\_\_ pce. of silt bucket(s)  delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |